<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.3-Bratislava">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["MEXICO_ITRF_2008_LCC",BASEGEOGCRS["GCS_MEXICO_ITRF_2008",DATUM["International Terrestrial Reference Frame 2008",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]],ID["EPSG",1061]],PRIMEM["Greenwich",0,ANGLEUNIT["Degree",0.0174532925199433]]],CONVERSION["unnamed",METHOD["Lambert Conic Conformal (2SP)",ID["EPSG",9802]],PARAMETER["Latitude of false origin",12,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Longitude of false origin",-102,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of 1st standard parallel",17.5,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",29.5,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Easting at false origin",2500000,LENGTHUNIT["metre",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",0,LENGTHUNIT["metre",1],ID["EPSG",8827]]],CS[Cartesian,2],AXIS["easting",east,ORDER[1],LENGTHUNIT["metre",1,ID["EPSG",9001]]],AXIS["northing",north,ORDER[2],LENGTHUNIT["metre",1,ID["EPSG",9001]]]]</wkt>
      <proj4>+proj=lcc +lat_0=12 +lon_0=-102 +lat_1=17.5 +lat_2=29.5 +x_0=2500000 +y_0=0 +ellps=GRS80 +units=m +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>MEXICO_ITRF_2008_LCC</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378137:6356752.31414035614579916</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
